**Known Issues**

The following are the known issues in this version of DynaLift TM version 4.1:

* On the *Well Identification* screen, the ***Date*** being populated for models files is not saved.
* When using *Unload Destination* as *Pit*, application hangs. The issue has been noticed in DynaLift version 3.6 too.
* Unit conversion for *Formation Volume Factor* does not work. This is an issue with epLibrary.
* In Windows 7, the user should have administrator privileges to run and view the simulation.
* We are not supporting unit conversion for Deviation survey, Equipment and Valve data section.
* Scrolling issue in Wellbore deviation section.

**WellFlo Setup**

* Install latest WellFlo setup on test machine.
* Copy Dictionary.ENU.xml from the Language folder to C:\Documents and Settings\<<username>>\Local Settings\Application Data\Weatherford\Dynalift\ on the test PC.

**Features Supported:**

* Loading existing model (DynaLift (.kdl;.kdlx) and WellFlo (.wflx)
* Modification and Saving model
* Creation of new Model
* Calculation of PVT Results
* Continuous Simulation
* Animation
* License – Proper DynaLift and Valve licenses are required to run the application.

**Features not supported**

* Intermittent Simulation
* Localization

**Features Supported:**

* Loading existing model (DynaLift (.kdl;.kdlx) and WellFlo (.wflx)
* Modification and Saving model
* Creation of new Model
* Calculation of PVT Results
* Continuous Simulation
* Animation
* License – Proper DynaLift and Valve licenses are required to run the application.

**Features not supported**

* Intermittent Simulation
* Localization